|  |  |  |  |
| --- | --- | --- | --- |
| Name of Assessor |  | Date |  |
| Name of Cleaning Operative |  | Date |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Persons Exposed | Injury Potential | Proposed Remedial Action | Applicable | Non Applicable |
| Public  Cleaning Operatives | Medium to High | Erect signs at all entrance, access points to indicate work in progress.  2. Keep equipment stored in a safe secure location, or during operation place in an area away from access points.  3. Keep cables from crossing over any access areas, in such instances cables must be secured or taped down to prevent tripping possible.  4. Floor stripping and resealing - Complete isolation of area to be implemented, no access to be permitted during operation to any personnel area other than cleaning operatives.  5. Display all warning signs until floors are dry. |  |  |

I have been given adequate training to use all of the above mentioned chemicals and machinery, And I understand this Risk Assessment.

Version 1 – Risk Assessment 3 Issue Date: August 2009 Pages 1 of 1