**BOURNE PROPERTY MAINTENANCE LTD **

**RISK ASSESSMENT 7**

**Steam Cleaning**

|  |  |  |  |
| --- | --- | --- | --- |
| Name of Assessor |  | Date |  |
| Name of Cleaning Operative |  | Date |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Operations | Risk Identified | Proposed Remedial Action | Applicable | Non Applicable |
| Burn and Scalding | Low | Ensure operative is wearing P.P.E clothing.Do not touch point of contact of steam hood. |  |  |
| Inhalation of SteamBurn to lungs | None | None. Dry steam is only at 180 degrees Celsius on point of contact. |  |  |
| Electric ShocksOver loading of Power | Low | Unwind all cables.Observe control panel. |  |  |
| Slip, Trip and Falls | Low | Tape down power supply cables, work with equipment behind operative. Work from furthest point towards exit. |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

I have been given adequate training to use all of the above mentioned chemicals and machinery, And I understand this Risk Assessment.

Version 1 – Risk Assessment 7

Issue Date: August 2009 Pages 1 of 1